# Safety Look-Out Training and Responsibilities

1. The Safety Look-Out assists the Safety Driver with Safe Operation of the Vehicle
   * Ensuring the safety of the people in and around the vehicle, the vehicle itself and the facility
   * Ensuring the area all around the vehicle is clear because the Safety Driver’s visibility is restricted
2. When Safety Driver shouts **“CLEAR”** that is when your responsibilities start

**Make sure:**

* You are outside standing outside the vehicle, not riding
* You remove the wheel chocks
* You unplug the vehicle charging cable
* There is nothing in the path of the vehicle
* Everyone is clear of the vehicle
* Everyone around is paying attention

1. Then reply by shouting **“READY”**

* However, your job still continues:
* Look out for people moving around
* Look out for other people/equipment entering the bay through doors, etc.

1. If at any time you think safety may be compromised **YELL** **“STOP”**
2. If Safety Driver doesn’t hear you or time is short – press one of the of the Emergency Buttons (Note: this does not stop the vehicle but only disengages the computer)
3. Upon normal completion of an experiment the Safety Driver then shouts **“OK”** people can then approach vehicle to discuss issues with the experiment and troubleshoot
4. The next experiment starts with Safety Driver shouting **“CLEAR”**